## +D Emulation

Fuse supports emulating the +D disk and printer interface. See the DISK FILE FORMATS section for more details on supported disk file formats. The +D's printer port is emulated. (See the PRINTER EMULATION section for more details.) The +D may only be used with 48K, 128K and +2 (not +2A) emulation. To access disks, load G+DOS, by inserting a disk containing the DOS file (+SYS) and entering "RUN". Once DOS is loaded, you can load to/from +D disks by prefixing filenames with `d n' where ` n ' is the number of the drive in use. For example, `LOAD d1;"myfile"' would load the file named `myfile' from the emulated drive 1. Microdrive syntax may also be used.

To save a snapshot, choose the `Machine, NMI' menu option, and then press `4' to save a 48K snapshot, or `5' to save a 128K snapshot.

When saving a 128K snapshot, you must then press Y or N to indicate whether the screen changed while saving the snapshot, to finish saving. You can also choose `3' to save a screenshot to disk.

Options `1' and `2' allow screenshots to be printed (in monochrome) if printer emulation is enabled.